**Karman Development Board Manual**

# Terms

Magnet Grades: A magnet grade is a good measure of the strength of a magnet. In general, higher numbers indicate a stronger magnet.

Pull Force: Pull force is how much force you have to pull on a magnet to move it away from something, such as a steel surface or another magnet.

# Mounting

2-56 screws should be used for mounting the DevBoard.

The diameter of the four mounting holes are set for 4-40 screw diameter. The diameter of the mounting holes are 0.0960 in.

# PCB Review

## Items to Check

## All power supply to ICs need to first pass through their decoupling caps.